## How to Update the Firmware of LOKLiK Crafter & LOKLiK iCraft

Update the firmware of the LOKLiK iCraft
Step 1:Click "Decice" - "Firmware Update" in LOKLiK IdeaStudio；

Step 2:Select Device - Click "Next"；

Step 3:Click "" to connect the device - Select the desired version to update；

Update the firmware of the LOKLiK Crafter

Step 1:Click "Device" - "Firmware Update" in LOKLiK IdeaStudio；

Step 2:Select Device - Click "Next"；

Step 3:Click "" to connect the device - Select the desired version and download the installation package；

Step 4:Press the machine's power button before clicking "Update" in LOKLiK IdeaStudio, and keep pressing the button during the update.
Notes：
·Keep pressing the power button while clicking "Update"；
·Do not release the power button or close the updating window until the system prompts you the updating is finished, or t he machine may not turn on properly；
·Please save your designs before updating；
·Ensure the machine and computer/notebook have ample power and stable internet connection during the update；
·If your software is version 1.9.7 or later, please update the firmware version (version 0010), otherwise it will affect the use of Print-then-Cut and Machine Calibration functions!
If the firmware update fails:
Re-open the firmware update window, keep pressing the power button while connecting the device via USB and re-updating the firmware. Or use the LOKLiK IdeaStudio flush tool to perform firmware updates

CONTACT US